## General Logics

The input epw is:

https://ibis.geog.ubc.ca/~achristn/research/BUBBLE/data/BUBBLE\_AT\_IOP.txt

The output air temperature is: <https://ibis.geog.ubc.ca/~achristn/research/BUBBLE/data/BUBBLE_BSPR_AT_PROFILE_IOP.txt>

UWG and VCWG may not receive preferential consideration in the building performance validation. They'll assume the building model is fine as long as the expected canyon temperature matches.

Based on the summarized thermal properties in UWG (Bueno et al., 2013) paper, (Bueno et al., 2013) and (Moradi et al., 2021, 2022) declaimed that building characteristic in the BUBBLE campaign (Rotach et al., 2005) should be modified based on the post-80s’ mid-rise apartments reference building model (*Commercial Reference Buildings*, n.d.).

## Thermal Properties Comparison

A picture containing text

Description automatically generated

## Replicated and Refining Validation

Maximum Daily UHI effect: 5.2 K

UWG Monthly MBE: -0.6, RMSE: 0.9

Bias Mean(K), RMSE(K), R2(-)

VCWGv2.0.0 MBE: -0.53, RMSE: 0.56, R2: 0.98

('VCWG(v200)-Real Temperature error', -0.26, 0.69, 0.94)

('VCWG(EP-Reference)-Real Temperature error', 0.18, 0.79, 0.93)

('VCWG(EP-Refining)-Real Temperature error', 0.23, 0.67, 0.95)

Chart

Description automatically generated

## References

Bueno, B., Norford, L., Hidalgo, J., & Pigeon, G. (2013). The urban weather generator. *Journal of Building Performance Simulation*, *6*(4), 269–281. https://doi.org/10.1080/19401493.2012.718797

*Commercial Reference Buildings*. (n.d.). Energy.Gov. Retrieved May 30, 2022, from https://www.energy.gov/eere/buildings/commercial-reference-buildings

Moradi, M., Dyer, B., Nazem, A., Nambiar, M. K., Nahian, M. R., Bueno, B., Mackey, C., Vasanthakumar, S., Nazarian, N., Krayenhoff, E. S., Norford, L. K., & Aliabadi, A. A. (2021). The Vertical City Weather Generator (VCWG v1.3.2). *Geoscientific Model Development*, *14*(2), 961–984. https://doi.org/10.5194/gmd-14-961-2021

Moradi, M., Krayenhoff, E. S., & Aliabadi, A. A. (2022). A comprehensive indoor–outdoor urban climate model with hydrology: The Vertical City Weather Generator (VCWG v2.0.0). *Building and Environment*, *207*, 108406. https://doi.org/10.1016/j.buildenv.2021.108406

*Reducing Energy Costs and Peak Electrical Demand Through Optimal Control of Building Thermal Storage | Applied Energy Science—ESDR*. (n.d.). Retrieved August 6, 2022, from https://appliedenergyscience.lbl.gov/publications/reducing-energy-costs-and-peak

Rotach, M. W., Vogt, R., Bernhofer, C., Batchvarova, E., Christen, A., Clappier, A., Feddersen, B., Gryning, S.-E., Martucci, G., Mayer, H., Mitev, V., Oke, T. R., Parlow, E., Richner, H., Roth, M., Roulet, Y.-A., Ruffieux, D., Salmond, J. A., Schatzmann, M., & Voogt, J. A. (2005). BUBBLE – an Urban Boundary Layer Meteorology Project. *Theoretical and Applied Climatology*, *81*(3), 231–261. https://doi.org/10.1007/s00704-004-0117-9